***LNGC 95253/17 (Refrigerated LNG Carrier 170000 cbm)******-------------******95,253 mtdwat on 12.522 m Summer Seawater Draft******Built  2017 in S.Korea
DNV-GL Class (+)1A1 Tanker for liquefied gas BIS BWM(T) Clean
COAT-PSPC(B) E0 Gas fuelled NAUT(OC) NAUTICUS(Newbuilding) TMON
Special Survey due 2.2027
Bahamas Flag. Port of Registration: Bahamas

Size: 294.90 oa / 282.90 pp x 46.40 x 26.50 m******Tonn: 117535.92 GT / 104298.90 NT (Suez: 117535.92/104298.90)*** ***LDT : 35,851.5 metric tons Lightweight******--------------------------------------******Bridge/Engine Room: Aft. Bulbuous Bow, Double Hull
KTM (Keel to Top of Mast): 59.11 m
Max Airdraft in Ballast: 49.56 m
Conditions of Carriage: GTT N0.96
Nr. of Independent Cargo Tanks: 4 (four)*** ***Cargo Tank Cubic Capacity: 173,560.0 cbm (100%)
Minimum Temperature: - 163 Degrees Celsius
Max Pressure: 25.0 kpa
Cargo Pumps: 2 per tank x Shinko Centrif. x 1750 m3/h x 160 m
Stripping pp: 1 per tank x Shinko  Centr. x 60 m3/hr x 140 m
Auxiliary pp: 2 x LNG HP Pump, A Cryogenic x 12 m3/h x 126 m
Emergency pp: 1 x Shinko x 550 m3/h x 150 mlc
Hose Handling: 2 Deck Cranes x 10 t SLW
Other Cranes: 2 x provision Cranes x 10t + 1 Compressor R.Cr.
Inert gas generation: Wartsila Moss AS - 16,000 Nm3/h
Bunkers: IFO: 3962 mt / MDO: 602 mt
Ballast Water Tanks: 61,924 m3 served by 3 pumps x 3100 m3/h
FW Generators: 2 x 25 m6/day f.237m3(ps tk) and 103m3 stb tk)
--------------------------------------------------------------***

***Main Engines: 2 × MAN B&W 5G70ME-C9-GI x ttl 24745 BHP/83 rpm
Propellers  : 2 x Cu-NiAl Bronze x Fixed Pitch Type******Diesel-Gens : 2 x Wartsila 6L343DF x 3912 Kw + 2 x 2610 Kw AC
Max trial sp: 20.7 knots
Speed/Consum: 19.5-18.5-17.5-12 knots on 109.7/94.2/84.2/45.4 t
MDO Consumpt: 0.55-0.60 per day
----------------------------------------------------------------******Vessel reported as in excellent condition for her age.******She is usually trading worldwide.

Sellers may consider a fairly prompt delivery******Pricewise Sellers inviting best outright offers as is/where is******and as brokers can guide accurately on price and furnish******you with full technical information, to named buyers with******background information disclosed.***

